Canadair CL415 information


Total aircraft weight with full fuel
           43,850 lbs.

          

VA - Manouvering Speed 		
		145 mph IAS
         
VFE - Maximum Flaps Extended Speed
		10° 159 mph IAS
           	25° land & Water operation 131 mph IAS

VNO - Maximum Structural Cruising Speed
            	233 mph IAS

VLE - Maximum speed Landing gear extended
		148 mph IAS

VS  -  Stalling Speed Flaps Up
          	86 mph IAS

VSO - Stalling Speed Flaps Landing
         	75 mph IAS



NOTE:  For explanations of speeds used on this tab, see "V-speeds" in the Glossary section of Help.
