[lists]
0=Cockpit Prep
1=Crew at Stations
2=Before Engine Start, BEFORE START Checklist
3=After Engine Start, AFTER START Checklist
4=Taxi Check, TAXI CHECK Checklist
5=Before takeoff, BEFORE TAKE-OFF Checklist
6=Climb, CLIMB Checklist
7=Descent, DESCENT Checklist
8=Approach, APPROACH Checklist
9=Final, FINAL Checklist
10=After Landing, AFTER LANDING Checklist
11=Parking, PARKING Checklist

[0]
1=PINS AND COVERS ON BOARD
2=EMERGENCY EQUIPMENT     ON BOARD / CHECKED 
3=CIRCUIT BREAKERS        CHECKED 
4=BATTERY MASTER, AC/DC   ON 
5=DC POWER CONTROLS       SET / CHECKED 
6=DC EXTERNAL POWER       AS REQUIRED 
7=BUS TIE CLOSED 
8=DOCUMENTS AND FORMS     CHECKED 
9=LANDING GEAR EMERGENCY EXTENSION SYSTEM CHECKED 
10=DEICE / ANTI-ICE SYSTEMS        OFF 
11=FIRE WARNING    TESTED 
12=FUEL OFF HANDLES        TESTED / IN 
13=SMOKE WARNING   TESTED 
14=ELT     AUTO 
15=FLIGHT DATA RECORDER / COCKPIT VOICE RECORDER   TESTED 
16=IGNITION        NORMAL 
17=AUX PUMPS       OFF 
18=ENGINE START SELECTOR   OFF 
19=FUEL TRANSFER   OFF / CLOSED 
20=PRESSURIZATION  SET 
21=EXTERIOR LIGHTS AS REQUIRED 
22=AC POWER CONTROLS       SET / CHECKED 
23=AIR CONDITIONING CONTROLS       SET 
24=NO SMOKING SIGN ON 
25=EMERGENCY LIGHTS        CHECKED / ARMED 
26=ANTI-SKID       ON 
27=SYNCHROPHASE    OFF 
28=CLOCKS  SET 
29=CAUTION / ADVISORY LIGHTS       TESTED 
30=GPWS    TESTED 
31=PFC SHUT OFF SWITCHLIGHTS       NORMAL 
32=SPOILERS        TAXI 
33=STBY HORIZON    CHECKED 
34=HYDRAULIC SYSTEMS       CHECKED 
35=ENGINE INTAKE DEFLECTORS        RETRACTED 
36=AUTOFEATHER     OFF 
37=GEAR WARNING    TESTED 
38=ROLL SPOILER PRESSURE SWITCHES  NORMAL 
39=STATIC SELECTORS        NORMAL 
40=CONTROL DISCONNECT HANDLES      IN 
41=CONTROL LOCK    ON 
42=GYRO CONTROL PANELS     CHECKED 
43=TRANSPONDER     OFF 
44=DME     ON 
45=AVIONICS COOLING SWITCH AUTO 
46=FLIGHT IDLE GATE        OUT 

[1]
0=PREFLIGHT INSPECTION & SYSTEM CHECKS    COMPL. / 1=CHECKED 
2=PINS AND COVERS REMOVED 
3=AIRCRAFT LOG & OPEN ITEMS       CHECKED 
4=OXYGEN MASKS & QUANTITY CHECKED 
5=PARK BRAKE AND PRESSURE SET / CHECKED 
6=TRIM TABS       3 SET 
7=ALTIMETERS      CROSS-CHECKED 
8=FUEL QUANTITY   TESTED / CHECKED 
9=AUTOPILOT SELECTOR      AS REQUIRED 
10=EMERGENCY BRIEFING     AS REQUIRED 
11=RADIOS  SET 

[2]
0=TAKE-OFF AND DEPARTURE PREPARATION      PEFORMED 
1=AUX HEATERS     OFF 
2=IGNITION        AS REQUIRED 
3=ANTI COLLISION LIGHT    RED 
4=SEAT BELT SIGN  ON 
5=FUELING ON CAUTION LIGHT        OUT 
6=DOOR WARNING LIGHTS     OUT 
7=POWER LEVERS    FLIGHT IDLE 
8=CONDITION LEVERS        FUEL OFF

[3]
0=START BUTTON / SELECTOR OFF / OUT 
1=IGNITION        NORMAL 
2=EXTERNAL POWER  OFF 
3=DC VOLTS / LOADS        CHECKED 
4=DEICE / ANTI-ICE SYSTEMS        SET 
5=BATTERY TEMPERATURES    CHECKED 
6=AIR CONDITIONING        SET 
7=SPOILERS        TAXI 
8=AUTOPILOT / YAW DAMPER  TESTED / ON 
9=FLIGHT INSTRUMENTS      CHECKED 
10=FLAPS   TAKE-OFF SETTING 
11=RUDDER TRAVEL   FREE / CORRECT 
12=RUDDER PUSH-OFF SWITCHES        TESTED 
13=ROLL SPOILER PUSH-OFF SWITCH    TESTED 
14=RADAR   STBY 
15=AUTOFEATHER     SELECTED 
16=DEICE SYSTEM PRESSURE   CHECKED 
17=HYDRAULIC PRESSURE      CHECKED 
18=NOSE WHEEL STEERING     ON 
19=CONDITION LEVERS        AS REQUIRED 
20=AC GENERATORS   AS REQUIRED 

[4]
0=TAKE-OFF BRIEFING       AS REQUIRED 
1=DEPARTURE       AS REQUIRED 
2=AC VOLTS / LOADS        CHECKED 
3=RADAR   TESTED 

[5]
0=CABIN   INFORMED 
1=CABIN REPORT    RECEIVED 
2=FLIGHT DIRECTOR SET 
3=CONDITION LEVERS        MAX 
4=CONTROL LOCK / CONTROLS OFF / CORRECT 
5=SPOILERS        FLIGHT 
6=DEICE / ANTI-ICE SYSTEMS        SET 
7=BLEEDS  OFF 
8=AC GENERATORS   ON 
9=CAUTION LIGHT PANEL     BLACK 
10=TRANSPONDER     SET 
11=GROUND RANGE LIGHTS     CHECKED 
12=CABIN CHIME     GIVEN 

[6]
0=ALTIMETERS      CROSS-CHECKED 
1=RADIO ALTIMETERS        MAX 
2=GEAR    UP 
3=FLAPS   0 / 0 
4=CLIMB POWER     SET 
5=DEICE / ANTI-ICE SYSTEMS        SET 
6=AUTOFEATHER     OFF 
7=BLEEDS & AIRCONDITIONING CONTROLS       SET 
8=PRESSURIZATION  CHECKED 
9=ENGINE INDICATIONS      NORMAL 
10=IGNITION        AS REQUIRED 
11=NO SMOKING SIGN AS REQUIRED

[7]
0=FASTEN SEAT BELT SIGN   ON 
1=PRESSURIZATION  SET / CHECKED 
2=FUEL TRANSFER   OFF 
3=FLIGHT IDLE GATE        CHECKED 
4=BRIEFING        AS REQUIRED 

[8]
0=ALTIMETERS      CROSS-CHECKED 
1=PARK BRAKE      OFF 
2=HYDRAULIC SYSTEMS       CHECKED 
3=PRESSURIZATION  CHECKED 

[9]
0=CABIN CHIME     GIVEN 
1=SYNCHROPHASE    OFF 
2=GEAR    DOWN / 3 GREENS 
3=FLAPS   15 / 15  OR  25 / 25  OR  45 / 45 
4=CONDITION LEVERS        MAX 

[10]
0=RADAR & TRANSPONDER     STBY / OFF 
1=CONTROL LOCK    ON 
2=FLAPS   AS REQUIRED 
3=SPOILERS        TAXI 
4=LANDING LIGHTS  OFF 
5=DEICE / ANTI-ICE SYSTEMS        OFF 
6=IGNITION        NORMAL 
7=ANTI-COLLISION LIGHT    RED 
8=AC GENERATORS   OFF 

[11]
0=TAXI LIGHT      OFF 
1=EMERGENCY LIGHTS        OFF 
2=RADAR   OFF 
3=EXTERIOR LIGHTS SET 
4=NOSE WHEEL STEERING     OFF 
5=CHOCKS  AS REQUIRED 
6=PARK BRAKE      AS REQUIRED 
7=EXTERNAL POWER  AS REQUIRED 
8=BATTERY MASTER, AC / DC OFF 
9=DC GENERATORS   OFF 
10=LEFT / RIGHT BATTERY    AS REQUIRED 
11=ANTI-SKID       AS REQUIRED 
12=ELT     AS REQUIRED 


